

1. After successful connection, the the board firmware information will on the the bottom left corner




1. Click on the upper right corner of the menu, select [update control panel firmware]




1. Select the firmware to update to ,



4. choose to update other firmware



1. After selecting the firmware, it will start to update. At this time, all the interfaces will be temporarily unavailable. Please wait while the small light on the board will flash rapidly



6.Wait a moment, it will be prompted to success, click ok, update the firmware is completed